**DEVELOP A PYTHON SCRIPT**

|  |  |
| --- | --- |
| Team ID | PNT2022TMID13652 |
| Project Name | Smart waste management system for metropolitan cities |

import requests

importjson importibmiotf.application import ibmiotf.device import time import random import sys

# watson device details organization "4yi0vc" devicType = "BIN1" deviceId = "BIN1ID" authMethod= "token" authToken= "123456789"

#generate random values for randomo variables (temperature&humidity)

def

myCommandCallback(cmd): global a print("command recieved:%s"

%cmd.data['command'])

control=cmd.data['command'] print(control) try:

deviceOptions={"org": organization, "type": devicType,"id": deviceId,"auth-

method":authMethod,"authtoken":authToken} deviceCli = ibmiotf.device.Client(deviceOptions) except Exception as e: print("caught exception connecting device %s" %str(e)) sys.exit()

#connect and send a datapoint "temp" with value integer value into the cloud as a type of event for every 10 seconds deviceCli.connect() while True:

distance= random.randint(10,70)

loadcell= random.randint(5,15) data=

{'dist':distance,'load':loadcell}

if loadcell < 13 and loadcell

> 15:

load = "90 %" elif loadcell < 8 and loadcell > 12: load = "60 %"

elif loadcell < 4 and loadcell > 7: load = "40 %"

else: load = "0 %"

if distance < 15: dist = 'Risk warning:' 'Dumpster poundage getting high, Time to collect :) 90 %' elif

distance < 40 and distance >16: dist = 'Risk warning:' 'dumpster is above 60%' elif distance < 60

and distance > 41: dist = 'Risk warning:' '40 %' else: dist = 'Risk warning:' '17 %'

if

load == "90 %" or distance == "90 %":

warn = 'alert :' ' Dumpster poundage getting high, Time to collect :)'

elif load == "60 %" or distance == "60 %":

warn = 'alert :' 'dumpster is above 60%' else :

warn = 'alert :' 'No need to collect right now '

def myOnPublishCallback(lat=10.678991,long=78.177731):

print("Gandigramam, Karur") print("published distance = %s " %distance,"loadcell:%s "

%loadcell,"lon = %s " %long,"lat = %s" %lat) print(load) print(dist) print(warn)

time.sleep(10) success=deviceCli.publishEvent ("IoTSensor","json",warn,qos=0,on\_publish=

myOnPublishCallback) success=deviceCli.publishEvent

("IoTSensor","json",data,qos=0,on\_publish= myOnPublishCallback) if not success:

print("not connected to ibmiot") time.sleep(30)

deviceCli.commandCallback=myCommandCallback

#disconnect the device deviceCli.disconnect

**Screenshots Python script:**

